//Probably useless reminder, but I write these manually, so this isn’t a makefile.

(In Directory)

**boot\_sect.asm to boot\_sect.bin (NASM)**

nasm boot\_sect.asm –f bin –o boot\_sect.bin

**kernel.c to kernel.bin (Command Prompt)**

gcc –ffreestanding –c kernel.c –o kernel.o

ld –T NUL –o kernel.tmp –Ttext 0x1000 kernel.o

objcopy –O binary –j .text kernel.tmp kernel.bin

**Create disc image (Command Prompt)**

copy /b boot\_sect.bin+kernel.bin os1.img